{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["Info","Trassid","Hydrandid","Kaevud","S6lmed","Sulgeseadmed","Reoveepumplad","Puurkaev_pumpla","Reoveepuhastid"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Info","index":0,"n_rows":2,"n_cols":11,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["ID","T88_nr","T88_nimi","Teostaja_nimi","Kontakt","M66distaja","CAD_faili_nimi","M66tkava","M66tmise_kpv","Vald","Asula"]
[1,"3-145-051","Vee- ja reoveevõrgustiku teostusjoonis","nn","Veski 69, Tartu","nn","1.3-145-05_teeaare_mu.dwg",0.3888888888888889,"2005-08-17","Ülenurme vald","Õssu küla"]

{"sheet":"Trassid","index":1,"n_rows":11,"n_cols":10,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["ID"," Kood","X","Y","Z","L2bim66t","Materjal","Otstarve","Ehitusaasta","M2rkus"]
[1,501,6472596.7193999998,655319.81980000006,55.33,110,"PE","Tänavatoru",2005]
[1,null,6472595.9554000003,655320.03899999696,0]
[1,null,6472582.1819000002,655330.37259999698,0]
[1,null,6472581.6491999999,655330.86990000005,55.68]
[2,501,6472581.6491999999,655330.86990000005,55.69,110,"PE","Tänavatoru",2005]
[2,null,6472581.5366000002,655330.97510000004,55.69]
[3,502,6472630.5718999999,655386.2548,0,160,"PVC","Tänavatoru",2005]
[3,null,6472633.6268999996,655384.81700000004,56.31]
[4,502,6472633.6268999996,655384.81700000004,56.28,160,"PVC","Tänavatoru",2005]
[4,null,6472599.0459000003,655317.20129999996,55.5]

{"sheet":"Hydrandid","index":2,"n_rows":4,"n_cols":10,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","Maapinna_Z","T2histus","Tyyp","Mark","Toru_l2bim66t","Ehitusaasta","M2rkus"]
[1,6472631.7966,655456.17769999802,55.1,"TH-10","Maapealne tuletõrjehüdrant",null,110,2005]
[2,6472315.7766000004,655612.30650000297,55.1,"TH-11","Maapealne tuletõrjehüdrant",null,110,2005]
[3,6472459.1809999999,655429.67890000297,55.1,"TH-12","Maapealne tuletõrjehüdrant",null,110,2005]

{"sheet":"Kaevud","index":3,"n_rows":4,"n_cols":21,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["ID"," Kood","X","Y","Maapinna_Z","P6hi","Kaane_l2bim66t","Kaane_materjal","Kaane_tyyp","Kaane_k6rgus","Kaevu_l2bim66t","Kaevu_materjal","Kaevu_tyyp","M2rkus","Ehitusaasta","Toru1","Toru2","Toru3","Toru4","Toru5","Toru6"]
[1,509,6472594.3919000002,655320.86230000097,57.46,55.47,null,"Metall","Kinnine",57.33,"560/500","Plast",null,null,2005,"55.47 De160 PVC","55.47 De160 PVC","55.60 De160 PVC"]
[2,509,6472599.0459000003,655317.20130000298,57.45,55.5,null,"Metall","Kinnine",57.37,"400/315","Plast",null,null,2005,"55.50 De160 PVC","55.50 De160 PVC"]
[3,509,6472580.7350000003,655331.03390000004,57.48,55.74,null,"Metall","Kinnine",56.91,"400/315","Plast",null,null,2005,"55.74 De160 PVC","55.75 De160 PVC","55.75 De160 PVC","55.94 De160 PVC"]

{"sheet":"S6lmed","index":4,"n_rows":4,"n_cols":11,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["ID","Kood","Otstarve","X","Y","K6rgus","Maapinna_Z","Ehitusaasta","M2rkus","Skeemi_nr","L2bim66t"]
[1,515,"sadul",6472581.6491999999,655330.86990000296,55.69,57.1,2005,null,11,"110/32"]
[2,515,"sadul",6472581.5366000002,655330.97510000295,55.69,57.1,2005,null,12,"110/32"]
[27,515,"kolmik",6472311.8348000003,655612.33070000296,54.1,55.4,2005,null,"10A"]

{"sheet":"Sulgeseadmed","index":5,"n_rows":4,"n_cols":9,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","K6rgus","Maapinna_Z","Tyyp","Otstarve","M2rkus","Ehitusaasta"]
[1,6472577.8781000003,655326.67800000298,55.58,57.48,"Maakraan","Majaühenduse kraan",null,2005]
[2,6472584.2784000002,655334.77799999702,55.69,57.59,"Maakraan","Majaühenduse kraan",null,2005]
[3,6472552.0643999996,655347.33269999898,56.11,58.01,"Maakraan","Majaühenduse kraan",null,2005]

{"sheet":"Reoveepumplad","index":6,"n_rows":2,"n_cols":24,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","K6rgus","Pumpla_nimi","Pumpla_tyyp","Pumpla_v6imsus_m3_d","Pumpla_ehitusaasta","Pumpade_arv","1_pump_pumpamisv6imsus_m3_h","1_pump_t6stek6rgus_m","1_pumba_mark","1_pump_ehitusaasta","2_pump_pumpamisv6imsus_m3_h","2_pump_t6stek6rgus_m","2_pumba_mark","2_pump_ehitusaasta","3_pump_pumpamisv6imsus_m3_h","3_pump_t6stek6rgus_m","3_pumba_mark","3_pump_ehitusaasta","Signalisatsioon","Kaugjuhitav","M2rkus"]
[1,6472590.6610000003,655316.53599999996,null,"RKP",null,null,2005]

{"sheet":"Puurkaev_pumpla","index":7,"n_rows":2,"n_cols":18,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","K6rgus","Puurkaevu_tyyp","Astmelisus","Puurkaevu_nimi","Passi_katastri_number","Puurkaevu_tootlikkus_m3_d","Pumba_t6stek6rgus_m","Pumba_v6imsus","Pumba_tootlikkus_m3_d","Pumpade_arv","Kaugjuhitav","Signalisatsioon","Veet88tlusega","Puurkaevu_ehitusaasta","M2rkus"]
[1,6472272.2999999998,655573.51280000003,null,null,"II astme","Õssu VTJ",null,null,null,null,null,null,null,null,"Jah",null,"puurkaev-pumpla-vtj"]

{"sheet":"Reoveepuhastid","index":8,"n_rows":2,"n_cols":20,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","K6rgus","Biotiik","Yhtlustusmahuti_x_m3","L2mmastiku_mahuti_x_m3","Aeratsioonimahuti_x_m3","J2relsetiti_x_m2","Mudatihendi_x_m3","Aktiivmudapuhasti_l2bivooluga","Aktiivmudapuhasti_SBR","Nimi","J6udlus","Kaugjuhitav","Septik","Signalisatsioon","Tyyp","Ehitusaasta","M2rkus"]
[1,6471127.1207999997,653323.84699999995,null,null,null,null,null,null,null,null,null,"Haage reoveepuhasti"]